// ****************************************************************************
//
// jlink-ota.txt
//
// J-Link Commander script for assisting with OTA programming.
//
// To use with J-Link Commander from a Command Prompt.
//  jlink  jlink-load_cm4_ble_v1p6p1.txt
//
// ****************************************************************************

// ****************************************************************************
//
//  Copyright (c) 2026, Ambiq Micro, Inc.
//  All rights reserved.
//
//  Redistribution and use in source and binary forms, with or without
//  modification, are permitted provided that the following conditions are met:
//
//  1. Redistributions of source code must retain the above copyright notice,
//  this list of conditions and the following disclaimer.
//
//  2. Redistributions in binary form must reproduce the above copyright
//  notice, this list of conditions and the following disclaimer in the
//  documentation and/or other materials provided with the distribution.
//
//  3. Neither the name of the copyright holder nor the names of its
//  contributors may be used to endorse or promote products derived from this
//  software without specific prior written permission.
//
//  Third party software included in this distribution is subject to the
//  additional license terms as defined in the /docs/licenses directory.
//
//  THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
//  AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
//  IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
//  ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE
//  LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
//  CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
//  SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
//  INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
//  CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
//  ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
//  POSSIBILITY OF SUCH DAMAGE.
//
//  This is part of revision stable-002b3c8e45 of the AmbiqSuite Development Package.
//
// ****************************************************************************

//
// Connect to the device.
//
usb
device AP510DLA-CBR
si SWD
speed 4000
r
sleep 100
h

// **** Change this based on device flashmap ****
// Load the OTA image at a temp place in flash
//
loadbin cm4_ble_v1p6p1_ota.bin 0x530000 noreset

// Set up OTA Descriptor at 0x43C000
//
w4 0x43C000 0x530003
w4 0x43C004 0xFFFFFFFF

// Set up OTAPointer
//
w4 0x4000AA64 0x43c001

// Reset - POI needed for reloading INFO0.
//
w4 0x40000004 0x1B

sleep 3000
connect

// Dump OTA Pointer - Should be 0x530000
mem32 0x43C000 1
// read CM4 INFO1 fields (00010200 01060001 005B8000 005FFFFF)
mem32 0x42003400 4

qc
